diff --git a/enforcement-case-studies.tex b/enforcement-case-studies.tex
index 793b53a71d64bca2549b93854e3bfd0ce09988ec..4da645b583e343172b0992d2a6d1c43432918e93 100644
--- a/enforcement-case-studies.tex
+++ b/enforcement-case-studies.tex
@@ -446,7 +446,7 @@ This instruction actually goes above and beyond the requirements of GPL\@.
 Specifically, the instruction guides users in their first step toward
 exercising the freedom to modify the software.  While the GPL does contain
 requirements that facility the freedom to modify (such as ensuring the CCS is
-in the ``preferred form \hellip for making modifications to it'' form, it
+in the ``preferred form \ldots for making modifications to it'' form, it
 does not require that you write specific instructions explaining how
 modifications might be undertaken.  This instruction therefore exemplifies
 the exceptional quality of this particular CCS\@.
@@ -570,7 +570,7 @@ chose the ``sysupgrade'' version of the image because this was clearly a
 system upgrade (as a firmware already came preinstalled on the
 TPE-NWIFIROUTER).
 
-Upon clicking ``Flash image\hellip'', the web interface prompted the
+Upon clicking ``Flash image\ldots'', the web interface prompted the
 investigator to confirm the MD5 hash of the image to flash.  The investigator
 did so, and then clicked ``Proceed'' to flash the image.  The process took
 about one minute, at which point the web page refreshed to the login screen.
